C     TEST DIPOLE USING NEW DATA INPUT FORMAT FOR GEOMETRY
C      WITH NEW FORMAT FOR NEAR FIELD DATA
C
WIRE(RADIUS=.01)
GROUND(HEIGHT=10/POOR)
GXYZ
0    0.5   0.1
1    0.4    0.2
2    0.3  0.3
XXXX
DNODE
1 2
2 3
XXXX
FEED(2)
FREQ(75)
PLOT(FARF/THETA=90)
OUTPUT(CURRENT/FARF=45,50,25,50)
NEAR
1.1  1.8   2.6
3.5    6.7 2.67  / The irregular spacing in this example
23.897  1   34.3  / illustrates the free format that can be used
XXXX
STOP
